Transmission mechanism Blocking of the output
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Blocking of the output detected. Effects on the driving operation The transmission shifts to neutral. Operating mode 'Waiting for neutral' Possible causes The computed vehicle retardation has reached implausible high values which may suggest blocking of the output. Place of action No description available. Instruction Check whether output is still permanently blocked. If there is no mechanical defect, no actions required. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)