Evaluation of brake request Inadmissible brake pedal combination in dataset
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Inadmissible brake switch combination in data batch. Effects on the driving operation Operation mode 'forced neutral'. Driving is not possible. Possible causes Brake switches are activated in the dataset constant RET_REQUEST_SOURCES_ which are mutually exclusive. (3-stage foot brake pedal and continuously variable foot brake pedal) Place of action No description available. Instruction Correct data batch value RET_REQUEST_SOURCES_ or load correct data batch. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)