Output signal BSB-OUT ( bus stop brake out ) Dataset fault in the signal assignment to one output
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Dataset fault in the signal assignment to an output of the E300. Effects on the driving operation ANS-variant with HSB activation not possible. Possible causes The configuration of the dataset value FLEXO_BSB_OUT_SETTING_ is incorrect. Place of action No description available. Instruction Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)