CAN gear range selector E330 The neutral no-signal is active.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description An error has been detected while monitoring the neutral-not signal: The neutral-not signal is active for too long without a button applied Effects on the driving operation No restrictions Possible causes Moisture has penetrated into the gear range selector. Gear range selector defective. Place of action No description available. Instruction Clear fault and apply neutral at the gear selector and wait for approx. 5 seconds. If the fault is re-entered, replace the gear range selector! Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)