Brake switch signal source hand brake switch 3-stage Supply line of brake switch input 3 interrupted
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Supply line of brake switch input 3 interrupted Effects on the driving operation No description available. Possible causes Cable break in plug connection, cabling or brake switch. Place of action No description available. Instruction Check plug connections, cabling and brake switch. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Troubleshooting for cable break
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)