Transmission oil temperature sensor E300.1 Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | See also:
Description Unknown fault. Effects on the driving operation Unable to detect temperature, possible consequences: Hard shifts with transmission oil cold. The temperature-related deactivation of the retarder is restricted. Possible causes The cause might be a cable break or short-circuit to supply voltage. If the error 'Reference voltage too high' is also present, this indicates a short-circuit to supply voltage. If only one temperature sensor reports this error, there might be a cable break at this sensor. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Check plug connections, cabling and sensor. Setting conditions for the event No description available. Test conditions for the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)