CAN-pushbutton switch E330 Short-circuit at the output FLEXO-HI-0
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description A circuit was detected at flexible output FLEXO-HI-0 of the gear range selector. It may be overloaded. The current may be max. 0.5 A. Effects on the driving operation The flexible output FLEXO-HI-0 is non-functional. Possible causes Short-circuit to ground at the flexible output. Overload. (current load of the output greater than 0.5A). An external voltage acts on the flexible output. Place of action No description available. Instruction Check cabling at flexible output FLEXO-HI-0 for short-circuit or external voltage. Measure the load current: The current load of the output must be smaller than 0.5A. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)