Operating data Resetting of the operating data via an external diagnosis command
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | See also:
Description Resetting of the operating data via an external diagnosis command. Effects on the driving operation No system response. Possible causes Deliberate clearing of the so far cumulated operating data using an external diagnostic tester. Location No location. Instruction No further actions required. Setting conditions for the event No description available. Test conditions for the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)