Kickdown No ADC value for kickdown signal available
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description No ADC value for kickdown signal available. Effects on the driving operation No kickdown active, hence no kickdown shifting points. Possible causes A fault has occurred inside the controller e.g.: - Timing problems in the control software. - Hardware faults in the ADC or multiplexer modules. Place of action No description available. Instruction If the fault occurs repeatedly, load updated software. Only if this measure remains without success, replace the control unit. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)