CAN brake signal source Brake pedal permanently applied
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Brake pedal permanently applied. Effects on the driving operation No ANS. No engaging of gears. No retarder function by brake pedal. Possible causes The brake pedal position received via CAN has never shown a released brake pedal in the current operating cycle although it can be assumed that the vehicle was not permanently braked. Possible causes are: * Defect at the brake switch that permanently leads to a too great brake pedal position. * The sending control unit delivers a too great brake pedal position. Place of action No description available. Instruction Check whether the brake switch provides a pedal position '0'. Check the CAN-message and contact the manufacturer of the sending unit if necessary. (With SAE J1939 see EBC1(Electronic Brake Controller #1), 'brake pedal position' ). Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)