Start page To favorites Print page |

### Event Monitor / Event Memory Monitor

In the Online Monitor window, the status of the event memory and a connected transmission controller is read and displayed at intervals. For monitoring specific events, you can either delete individual entries from the event memory or delete the entire event memory. You can also reset the transmission controller.

## Valid platforms:

- DIWA.3 via E200
- DIWA.3 via E310
- DIWA.5
- DIWA.6 via KWP
- DIWA.6 via UDS
- VIAB
- DIWAhybrid E300.1
- DIWAhybrid M300

## How to open the Event Monitor

The Event Monitor is accessed via the Service group in the main window. Then select the Event Monitor button in the Service menu.

The Event Monitor is offered depending on the connected ECU. The Event Monitor is not available without communication.

The display changes automatically after you have started the communication.

## How to use the Event Monitor

The Event Monitor reads the fault memory approx. once per second.
In order to clear an individual fault, mark the entry in the list and press the "Clear individual event" button or press the "Del" key.
To clear the entire event memory, press the "Clear event memory" button.
Using the "Reset ECU" button causes a warm start of the controller.

The principle of active and passive events Fault codes / Event codes