Start page To favorites Print page |

### Visual outputs of the Voith gear range selector E330

Any faults that occur are indicated to the driver by the flashing of the gear range selector lights. Different flashing codes provide information about the type and priority of the fault. This function is available as of gear range selector version G01.03. The software version is indicated in the identification data in the ALADIN ECU report.

Fault type or priority | Flashing duration | Flashing keys | Flashing frequency | Ratio of lighting ON / OFF | Animation
CAN Fault The gear range selector has no communication on the CAN bus. (No connection between the gear range selector and transmission control unit) | Until ignition off | All | 1 Hz (once per second) | 1 / 1 |
Priority 1 Event (saved) The event memory of the transmission controller signals one priority 1 fault saved after the ignition was switched on. | 10 seconds | All | 2 Hz (twice per second) | 1 / 1 |
Priority 2 Event (saved) The event memory of the transmission controller signals one priority 2 fault saved after the ignition was switched on. | 10 seconds | All | 2 Hz (twice per second) | 1 / 1 |
Priority 1 Event (current) The transmission controller signals one currently active priority 1 fault. | Until ignition off | All | 2 Hz (twice per second) | 1 / 1 |
Priority 2 Event (current) The transmission controller signals one currently active priority 2 fault. | 10 seconds | All | 2 Hz (twice per second) | 1 / 1 |
Priority 6 Event (current) The transmission controller signals one currently active priority 6 fault. | Until ignition off or error no longer present | "N" button | 1 Hz (once per second) | 1 / 3 |
The transmission control unit refuses to accept the gear | As long as the button is depressed or until the gear is accepted | Pressed button | 1 Hz (once per second) | 1 / 1 |