CAN-pushbutton switch E330 Fault writing to configuration memory (EEPROM)
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description A fault has occurred while writing to the configuration memory (EEPROM). Writing is not possible or read back data are faulty. Effects on the driving operation Modifications to the gear selector configuration were not applied (response depends on the modified data). Possible causes Moisture has penetrated into the gear range selector. Gear range selector defective. Place of action No description available. Instruction Clear fault memory, shut off the vehicle and restart. Check whether the fault is re-entered. If yes: Replace gear range selector. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)