Safety computer AD conversion defective
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description AD conversion defective. The 0V test voltage for testing the analog multiplexer and the AD converter is above the allowed maximum value. Effects on the driving operation Driving is not possible. Possible causes Internal fault of the safety computer Internal fault of the control unit Place of action No description available. Instruction Clear event memory Should the fault reoccur, please contact the VOITH customer service. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)