CAN 1 - Hardware Invalid bit rate
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Invalid bit rate. Effects on the driving operation No CAN-communication via the CAN-controller 1 of the transmission control unit possible. Vehicle does not drive or only with restrictions. Possible causes Software error. The bit rate in the software of the transmission control unit does not correspond to the standard values 250 or 500. Place of action Software in the transmission control unit Instruction No description available. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)