Kickdown Implausible "kickdown active" via CAN
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Implausible "kickdown active" via CAN. Effects on the driving operation No kickdown active, hence no kickdown shifting points. Possible causes Kickdown active was detected while the position of the accelerator pedal is merely smaller than or equal 50 %. Possible causes are: - for CAN signals there may be an implausible value in the CAN message. Place of action No description available. Instruction Please make sure that both the accelerator pedal and the kickdown switch operate correctly. For CAN signals check the CAN message (for SAE J1939 EEC2,Electronic Engine Controller #2), CAN signal: 'kick down switch' .) Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)