CAN Protocol IES Timeout of CAN message ID 592
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Troubleshooting
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Timeout of CAN message ID 592. Effects on the driving operation ANS (automatic neutral at standstill) may not be available. Kick-down not available. Speed plausibility check non-functional, therefore driving may not be possible. Possible causes FMR controller defective or connection to FMR controller faulted. Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Check FMR controller and connection to FMR controller. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)