Retarder oil Overtemperature of the retarder oil
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description Overtemperature of the retarder oil. The temperature threshold set in the dataset value RET_REDUCTION_T_CONV_RANGE_[1] was exceeded. Effects on the driving operation The retarder is deactivated because of a too high oil temperature. Possible causes Oil temperature too high because of high ambient temperatures or high braking power. Location No description available. Instruction No further actions required. It is a normal operating state. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)