ANS (Automatic Neutral at Standstill) Dataset fault of the digital input "Bus stop brake request".
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
Description Dataset fault of the digital input "Bus stop brake request". Effects on the driving operation No ANS function Possible causes The assignment of the digital signal to an input of the E300 via the dataset is faulty. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Load correct dataset. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)