ANS (Automatic Neutral at Standstill) CAN signal if the roll-back inhibit is active or not does not contain any valid value.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
Description CAN signal if the roll-back inhibit is active or not does not contain any valid value. Effects on the driving operation No ANS function Possible causes Signal sent via the CAN bus is not valid or cannot be received. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Check the CAN message and contact the manufacturer of the transmitting control unit if necessary. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)