Analog-digital converter of E300 (ADC) ADC voltages faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description ADC voltages faulty. Effects on the driving operation Driving is not possible. Possible causes Faulted reference voltage. Location Transmission control unit Instruction If the problem reoccurs, contact the VOITH customer service and update the function software of the control unit (if necessary). Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)