CAN engine load source CAN signal engine nominal torque faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The CAN signal containing the information on the engine nominal torque is faulty. Effects on the driving operation No ANS. Hard shifts. Possible causes The CAN-message required to determine the engine nominal torque provides faulty values. This message exists only with IES-CAN. The message can be found in the IES-CAN documentation. The values causing the fault can be found in the system description. Place of action No description available. Instruction Check CAN message / CAN signal and initiate correction if applicable. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)