System information Time signal "year" faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Time signal 'year' within the CAN message 'Time/Date' faulty (CAN-SPN 964). Effects on the driving operation Entries in the event memory contain no or faulty 'Time/Date identification'. Possible causes An incorrect value for 'Year' within the CAN message 'Time/Date' was received (CAN-SPN 964). Place of action No description available. Instruction Check CAN-message 'Time/Date' on the CAN-bus and make it available if necessary (if CAN-SAE-J1939 protocol is used). Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)