CAN-pushbutton switch E330 While reading data from the gear range selector other data than those requested were sent.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description While reading data from the gear range selector other data than those requested were sent. Effects on the driving operation Identification data of the gear range selector may be faulty or not available. Possible causes Defect in the CAN controller of the gear range selector or transmission control unit. CAN communication disturbed. Software fault in the gear range selector or in the transmission control unit. Place of action No description available. Instruction Check gear range selector and transmission control unit. Check whether the fault reoccurs. Replace the software of the transmission control unit. Contact Voith. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)