Evaluation of brake request No brake pedal specified in dataset
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description No brake switch specified in dataset Effects on the driving operation Activating retarder not possible. If it is desired that Gearguard or ANS are activated via the brake pedal position, these functions are not available. Possible causes No brake switch is activated in the dataset constant RET_REQUEST_SOURCES. Place of action No description available. Instruction If it is intended that NO (retarder) brake request is evaluated, then: * Ignore the fault entry. Or else: * Correct the dataset or load an updated dataset. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)