CAN-pushbutton switch E330 Voltages at the inputs and/or output supply unreliable values.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description One or more voltages at flexible inputs and/or at the flexible output supply unreliable values (one or more values in CAN messages (InputValues0…2) are greater than 64 255). Effects on the driving operation The flexible inputs and the flexible output at the gear range selector are non-functional. Possible causes Transmission control unit defective. Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)