Evaluation of gear selection range CAN signals "Requested Gear" or "Requested Range" deliver fault identification.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The gear information of the gear range selector is incorrect: At least one of the CAN signals ´Requested Gear´ or ´Requested Range´ delivers a fault identification. With DIWA.5 ´Requested Gear´ serves to read the information on the driving direction; ´Requested Range´ is used to determine the allowed gear range. Effects on the driving operation Driving is not possible. The transmission shifts to neutral. The optional limp-home switch allows continuing the drive. Possible causes Defect of the Voith CAN gear range selector or defect of the MAN-FFR (vehicle control computer) for systems without Voith CAN gear range selector. The message TC1 is affected. Place of action No description available. Instruction Replace gear range selector. In vehicles with MAN-FFR (vehicle control computer), contact the manufacturer and replace the FFR or the gear range selector connected to it. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)