ANS (Automatic Neutral at Standstill) Undiagnosible fault at the digital input "ANS".
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
Description Undiagnosible fault at the digital input "ANS". Effects on the driving operation No ANS function Possible causes Short-circuit to ground in plug connections, cabling or sensor. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Please contact the VOITH customer service. Setting conditions for the event No description available. Test conditions for the event No description available.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)