Dataset The checksum of the dataset does not match the dataset.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Troubleshooting
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The checksum of the dataset does not match the dataset. Effects on the driving operation The release for activating the solenoid valves is cancelled (forced neutral). The vehicle can not be moved. Possible causes The dataset has been damaged. The permanent memory of the control unit (FRAM) is defective. Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Clear the fault memory and restart the control unit. Reload dataset. If the fault persists, contact the Voith customer service. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)