CAN gear range selector E330 Faulty voltages at the flexible output and the flexible inputs
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description All voltages at the flexible output and the flexible inputs may be faulty. Effects on the driving operation The flexible inputs and the flexible output at the gear range selector are non-functional. Possible causes Moisture has penetrated into the gear range selector. Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)