Software module Event memory Multiple reports of one fault type
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description A diagnostic object reports multiple messages for one fault type. The reported values for fault location and fault type are indicated in the system description. Effects on the driving operation Event memory does not work correctly. Possible causes Software fault. A diagnostic object was not correctly implemented. Place of action No description available. Instruction Load new software. Send control unit file to VOITH. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)