Coolant temperature sensor Sensor lines are short-circuited to each other
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
|  | See also:
Description Short-circuit of the sensor lines to each other Effects on the driving operation No retarder operation. Possible causes Short-circuit in the sensor or in the sensor cabling. Place of action No description available. Instruction Check plug connections, cabling and sensor. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly. See also:
|  | Troubleshooting a short-circuit of two signals
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)