Kickdown Dataset fault in the signal assignment of the digital kickdown input signal
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Dataset fault in the signal assignment of the digital kickdown input signal. Effects on the driving operation No kickdown active, hence no kickdown shifting points. Possible causes The assignment of the kickdown signal to an input in the dataset is faulty. Place of action No description available. Instruction Correct dataset value FLEXI_KD_SETTING_ or load the correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)