Speed sensor for sun gear 1 Poor signal frequency quality
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Poor frequency signal quality The individual measured pulse durations and/or periods vary more than allowed (no continuous signal) Effects on the driving operation Main pressure to maximum. Reduction of the engine torque to protect the transmission. Hard shifts Possible causes Extreme torsional vibrations. Installation position of sensor is not correct or the sensor is loose. The pulse-generator wheel has damages that may cause signal disturbance. The sensor malfunctions. Place of action Speed sensor N3 Instruction Check the installation position of the sensor (distance, tolerance position). Make sure that the sensor sits tightly. Ensure the correct function of the sensor. Check the pulse-generator wheel for damage. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)