Brake switch signal source hand brake switch 3-stage Implausible brake switch signal
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Implausible brake switch signal. Effects on the driving operation No retarder operation. Possible causes Implausible signal concerning the respective brake switch stage. The signal is constituted by the 3 brake switch input signals. Place of action No description available. Instruction Set brake switch to valid position and check the afulty signal including the 3 inputs. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)