Output signal RG-SIG ( reverse gear signal ) Line interruption at the reverse gear signal output
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
|  | See also:
Description Line interruption at the reverse gear signal output. Effects on the driving operation No activation or permanent activation of the reversing light (depending on the configuration in FLEXO_RG_SIG_SETTING_) Possible causes Interruption in a cable and/or plug connection. Place of action No description available. Instruction Check cables and plug connections Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly. See also:
|  | Troubleshooting for cable break
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)