CAN protocol SAE J1939 Wrong sequence of the packets of the message EC
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Troubleshooting
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Incorrect packet sequence in the CAN receive message 'Engine Configuration'. Effects on the driving operation Hard shifts may occur. Possible causes Engine control unit does not send the CAN message 'Engine Configuration' correctly in accordance with SAE J1939 standard. Error in the engine control unit. Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Check the engine control unit and CAN connection to engine control unit. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | CAN SAE J1939 Voith specifics (SW E300-D2.3.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300-D2.4.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300.1-D5.0.0.0)
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)