DK lockup clutch solenoid valve
|  | Terminal connection diagram
|  | Test steps
|  | Resistance characteristics
Terminal connection diagram Test steps Open S1 plug connection. a. Power winding: Measure resistance between contacts 37 and 52 or 53 of cable 1. RTarget = 11-20 Ω. b. Measuring winding: Measure resistance between contacts 51 and 31 or 49. RTarget = 5-10 Ω. If R = RTarget, continue with 4. Open S3. a. Power winding: Measure resistance between contacts K and A or B (cable harness) or DK and -UB (measuring cable). RTarget = 11-20 Ω. b. Measuring winding: Check resistance between contacts b and h or j (cable harness) or DKM and SENSE (measuring cable). RTarget = 5-10 Ω. Remove control cover. Open S4. a. Power winding: Measure resistance between pin contacts 4 and 2 of tab connector of DK solenoid. RTarget = 11 ± 0.7 Ω. b. Measuring winding: Measure resistance between pin contacts 3 and 1 of tab connector of DK solenoid. RTarget = 5.2 ± 0.3 Ω. Check resistance between contact 51 and vehicle ground at open plug connection S1. RTarget = ∞ Ω. Check resistance between contacts 51 and 37. RTarget = ∞ Ω. Check resistance between contact b (or DKM) and ground at open plug connection S3. RTarget = ∞ Ω. Check resistance between contacts b (or DKM) and K (or DK). RTarget = ∞ Ω. Check resistance between contacts 1 and 4 to ground at open plug connection S4. RTarget = ∞ Ω. Check resistance between contacts 1 and 4. RTarget = ∞ Ω. Resistance characteristics When measuring the coil resistances, please observe the dependence on the temperature. Simultaneously to the resistance measurement, the temperature of the solenoid enclosure has to measured, too, or estimated with utmost accuracy. Read the target resistance from the temperature resistance curve below, assuming the measured or estimated temperature, and compare it to the measured value. Operating coil Measure the resistance between pin 4 and pin 2. The operating coil is intact when the measured resistance deviates from the target resistance by no more than ± 1 Ω approximately. Measuring coil Measure the resistance between pin 1 and pin 3. The measuring coil is intact when the measured resistance deviates from the target resistance by no more than ± 0.5 Ω approximately. No resistance - no connection - must be measurable between the pins and the solenoid's housing; the resistance is infinitely great. Characteristics: A = operating coil B = measuring coil
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)