TIM - Transmission Identification Module Transmission data: Transmission generation number is wrong
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description Transmission data: Transmission generation number is wrong. Effects on the driving operation The transmission-specific data is wrong. The vehicle might drive with the wrong transmission configuration. The newly specified transmission generation number was not accepted. Possible causes The newly specified transmission generation number is wrong. Location Data in the TIM. Instruction The transmission generation number must correspond to an actually existing number. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)