CAN 1 - Hardware Send buffer overflow in transmission control unit
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Send buffer overflow in transmission control unit The pipeline for sending CAN messages of CAN controller 1 is full. Effects on the driving operation Vehicle does not drive or only with restrictions. Possible causes Software problem or no CAN1 communication via CAN controller 1 possible. Place of action CAN bus Instruction No description available. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)