Analog-digital converter of E300 (ADC) ADC channel faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description ADC channel faulty Effects on the driving operation Driving is not possible. Possible causes Faulty AD conversion of an ADC channel. (expert information: The value for an incorrect ADC channel was stored in the software’s ADC buffer. The cause is probably a timing problem in the software.) Place of action No description available. Instruction If the problem reoccurs, contact the VOITH customer service and update the function software of the control unit (if necessary). Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)