> # Fault codes / event codes The fault code is a hexadecimal number that contains encoded information on the fault location and fault type. This code informs the vehicle master computer, for example, whether and what type of event has occurred. At the same time, ALADIN uses this code, e.g., to display repair instructions. Fault code: 0x00000000 Fault code: 000000h (alternative notation) A complete fault code is comprised of the designation components system, fault location, fault location type and fault type. The components system, fault location and fault location type form the fault source. The fault code is usually displayed as a hexadecimal number (long value).
> System | 0 = Voith DIWA.5 automatic transmission 2 = VIAB 3 = DIWAHybrid |
> Fault location | The fault location / event location signalling an event. For example: speed sensor at transmission output |
> Fault location type | The fault location type indicates that the probable cause of the event can be found here. For example: speed sensor at transmission output. |
> Fault type | The fault type, e.g., short-circuit to earth at the connecting cable between sensor and transmission control unit. |
| Further topics:
More information on: FAQ More information on: Upload More information on: Report Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)