# Voith adapter for the diagnosis with ALADIN A K-line interface (level converter) is required for connecting the vehicle to the PC (ALADIN). It is available both with a USB interface and with a RS232 (COM1) port. In the vehicle, the K-line interfaces are equipped with a standardized K-line connector. Depending on the vehicle manufacturer, you might need an adapter connector in the vehicle.
| Available Voith adapter connectors:
> |  | MAN OBD2 adapter Adapter for connecting a K-line interface to an MAN OBD2 diagnostic interface. You can order this adapter under: order no.: 150.00252710.
> |  | MAN TEPS adapter Adapter for connecting a K-line interface to an MAN TEBs diagnostic interface. Diagnostic interface. You can order this adapter under: order no.: 150.00046710.
> |  | E300 / E300.1 intermediate adapter Adapter for connecting a K-line interface directly to an E300 / E300.1 transmission control unit. The existing cabling between the transmission control unit and the transmission is looped through. You can order this adapter under: order no.: 150.00108510.
> |  | E300 / E300.1 intermediate adapter with CAN Adapter for connecting a K-line interface directly to an E300 / E300.1 transmission control unit. The existing cabling between the transmission control unit and the transmission is looped through. The two CAN1 and CAN2 ports are also available. You can order this adapter under: order no.: 150.00108610.
| Further topics:
More information on: Connector pin assignment More information on: Setup More information on: K-line interfaces More information on: Power Management settings More information on: Voith customer service More information on: FAQ Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)