# Using the Recorder The Recorder is used to record and play back measuring files. To be able to perform measurements with the Recorder, you must connect your PC to a Voith control unit and turn the ignition on. For further information on connecting the vehicle to your PC, please refer to: K-line interfaces.
| How to open the Recorder:
Double-click the Recorder symbol on your Windows desktop . Alternatively, you can click the menu item: Start > Voith Turbo > Recorder in Windows.
| The small Recorder training course:
> The measuring data is displayed with virtual measuring instruments in the Recorder. The virtual instruments displayed are defined by the measuring file template that is used. All instruments displayed simultaneously form a so-called Panel. A measuring file template may include several panels that you can switch between during recording. All signals that have been defined in the measuring file template are always recorded. This is done regardless of whether the panel is currently displayed or not. You have two options of opening a measuring file template. Click this button in the toolbar: Record: . The Recorder automatically opens an appropriate measuring file template for the control unit. Alternatively, click the menu item: File > New. In both cases, communication with a connected control unit is established and the measuring data is displayed in the virtual measuring instruments. However, this data is not yet recorded. The Recorder is in the standby mode. Click the File > Open menu item. The dialog box "Open" appears. Several measuring file templates are displayed. Select a measuring file template and exit the dialog box with Open. If the selected measuring file template is not suitable for the connected control unit, a corresponding error message will be displayed. The currently selected panel is displayed with "FP1" in the toolbar. With the two small buttons next to it you can switch between the different panels. You can also call up the first 9 panels directly using the numeric keypad. As an alternative, the "Options" menu provides the commands for: Next Panel, Previous Panel and Select Panel. The measuring template file for DIWA.5 transmissions includes 3 panels.
> | You can also start the Recorder automatically by selecting a measuring file template in the Windows Explorer.
You must start the Record function to record measuring data. To do so, click the Record button in the toolbar: . Alternatively, click the menu item: Recorder > Record. The Recorder will then change from the standby mode to the recording mode. If you want to pause the measurement, click the Stop button . You can use the Record button to go back to the standby mode at any time. Once you have performed the measurement, you can save the recording. To do so, click File > Save as... in the menu. The dialog box "Save as" appears. Navigate to the required directory, assign the required file name and exit the dialog using the Save button. You can use this file for evaluating the measuring data in the Voith Analyzer.
| The Recorder menu:
> The Recorder menu includes the following menu elements: File, Recorder, O ptions and ? for the Online Help: The file functions:
> Function | Description | Shortcut
> New | Builds up communication to a connected control unit and opens an appropriate measuring file template automatically. | Ctrl+N
> Open | Opens a dialog box for selecting a measuring file template. | Ctrl+O
> Connect via Network | Establishes a network connection to a DIANA5 server. |
> Close | Stops communication with a control unit and exits the active measuring file template. |
> Save | Saves the current measuring data recording in the current measuring file. |
> Save as... | Saves the current measuring data recording in a new file. |
> Send as e-mail | The current measuring data recording is sent to an e-mail address. The address can be entered in the Program Properties. |
> Program Properties... | Opens the DIANA5 Setup. |
> XXX | The measuring file templates used last are offered for opening. |
> Exit | Exits the Recorder. |
> The Recorder functions:
> Function | Description | Shortcut
> Stop | Brings the Recorder to the Stop mode. | S
> Pause | Brings the Recorder to the Pause mode. | H
> Playback | Brings the Recorder to the Play mode. | P
> Record | Brings the Recorder to the Record mode. | R
> Trigger Active | Activates the trigger-dependent recording of measuring data. For further information, please see: Trigger functions. | T
> Trigger Properties | Opens the dialog box for the trigger list. For further information, please see: Trigger functions. |
> Delete Measurement | Deletes the current measuring data recording. |
> The options:
> Function | Description | Shortcut
> Next Panel | Switches the display of the virtual measuring instruments to the next panel. | +
> Previous Panel | Switches the display of the virtual measuring instruments back to the previous panel. | -
> Select Panel | Opens a list of all panels of the currently active measuring file template. You can select any panel. | F
> Insert Marker | Inserts a marker in the measuring file while the measuring data is being recorded. You can enter any name for the marker. | Space
> Marker List | Displays a list of all markers used including relative time indications. |
> Event List | This function is not available in this version. |
> Recording Details | Displays the recording details of the currently active measuring file. This includes the identification data and the fault memory. In addition, you can store your user data and any comments in the measuring file. |
> Start ECUViewer | Opens the ECUViewer window. For further information, please see: ECUViewer. |
> Timer | Starts a timer. |
> Open Template in TED | This function is not available in this version. |
| The Recorder toolbar:
> Symbol | Description | Shortcut
> | Opens the dialog box for selecting a measuring file template. | Ctrl+O
> | Saves the current measuring data recording in a new file. |
> | Exits the Recorder. |
> | Opens the "Recording Details" window that displays the identification data and the fault memory of the active measuring file. In addition, you can enter your user data and comments. For further information, please see: Recording Details. |
> | Opens the ECUViewer window. For further information, please see: ECUViewer. |
> | Inserts a marker in the measuring file while the measuring data is being recorded. You can enter any name for the marker. |
> | Displays the current recording time. |
> | Brings the Recorder to the Stop mode. | S
> | Brings the Recorder to the Pause mode. | H
> | Brings the Recorder to the Play mode. | P
> | Brings the Recorder to the Record mode. | R
> | Activates the trigger-dependent recording of measuring data. For further information, please see: Trigger functions. | T
> | Displays the currently active Recorder mode. |
> | Displays the currently active panel. You can use the up/down buttons to switch between the different panels. |
> | Displays the ECU device status. Lights up green if communication with a control unit is active, otherwise it lights up red. |
| Recorder modes:
> The current operating mode is always displayed in the Recorder status display. The table below shows all possible modes:
> Display | Description
> Stop | The Recorder has been stopped. The measuring values are not updated.
> Pause | The playback of the measuring file has been paused.
> Play | The measuring file is played back.
> Standby | The measuring data displayed is updated continuously. However, no recording is active.
> No Trg | The trigger is switched on. Recording will be started, as soon as the trigger condition has been met.
> Record | The measuring data displayed is recorded or a measurement that has been stopped will be continued.
| Further topics:
More information on: Measuring template files More information on: K-line interfaces More information on: Recording details More information on: ECUViewer More information on: Trigger functions More information on: Network functions Up > © by Voith Turbo GmbH & Co. KG send remarks to Gottfried.Graf@Voith.com (electronic department) or r.theilacker@voith.com (electronic department)