# Recorder measuring template files:
| Recorder measuring template files:
> The appropriate measuring template files are required for using the Recorder with different control units. The Recorder is therefore supplied with more than 30 different measuring template files. The most important are:
> Measuring template file | Application | Started automatically?
> DIWA2.D5T | DIWA.2 transmission with special E200 controller |
> DIWA3.D5T | DIWA.3 transmission with software version up to 18.20 |
> DIWA3Xtd.D5T | DIWA.3 transmission with software version up to 18.20 including WR duty factor and oil temperature |
> DIWA3_18_2x.D5T | DIWA.3 transmission with software version as from 18.20 |
> DIWA5.D5T | DIWA.5 transmission |
> RETARDER.D5T | Retarder with VERA control |
> AQUATARDER.D5T | Aquatarder with VERA control |
> RETARDERDP.D5T | Aquatarder with DigiProp control |
> AD.D5T | A/D measurements |
> ALTITUDE.D5T | Altimetry using air-pressure sensor |
> GPS.D5T | GPS measurements |
> CAN_SAEJ_TX.D5T | SAE-J1939 CAN transmission messages |
> CAN_SAEJ_RX.D5T | SAE-J1939 CAN receive messages |
> CAN_IES_TX.D5T | IES CAN send messages |
Up > © by Voith Turbo GmbH & Co. KG send remarks to Gottfried.Graf@Voith.com (electronic department) or r.theilacker@voith.com (electronic department)