# Display identification data in the report
| Identification data describes the elements that the entire DIWA.5 transmission system is composed of. This includes, among other things, the transmission, the control hardware and the software. Thus, it is possible to select the appropriate component in the event of changes (e.g., a new dataset for new vehicle requirements or service work). Every element of the transmission system has separate identification data that was assigned during production and cannot be changed subsequently.
| The identification data is divided into: control unit and component:
| Control unit:
> Control unit | Version | Material number | Date | Info |
> Hardware | E300.1 | 150.00001321 | 2006-06-19 | 36MHz V1 |
> Software | E300.1-D5.2.0.0 | 150.00261410 | 2006-09-29 |  |
> Dataset | E300.1-D5.2.0.0-08154701 | 150.00263201 | 2006-08-25 |  |
> Entire control system | ECU-E300.1-D5.2.0.0-08154701 | 150.08154701 | 2006-12-01 |  |
> Loader | F05.05.03-u |  |  |  |
The transmission control unit comprises of the hardware, the function software, a dataset and a Loader. Hardware, software and dataset form the entire control system.
| Hardware
| The hardware can be either an E300 or an E300.1 controller. The hardware identification data includes the hardware version, the appropriate material number and the manufacturing date. The system block (processor speed) is indicated as additional information. This data is entered during production and cannot be changed.
| Software
| The software identification data includes the software version, the appropriate material number and the manufacturing date. The software version name is always composed of the identifier for the supported hardware (E300 or E300.1-), D for a DIWA / N for a NOWA transmission and the version number (e.g., 5.2.0.0). The two last numbers must always be "0.0". If you load a new software to the transmission control unit, the software identification data is changed automatically.
| Dataset
| The dataset identification data includes the dataset version, the appropriate material number and the manufacturing date. The dataset version name is always composed of the identifier for the software version the dataset may be used with (E300.1-D5.2.0.0 - see software) and an 8-digit number for the dataset. The dataset number consists of a 6-digit identifier (e.g., 081547) and a 2-digit modification index (e.g., 01). If a change in the dataset should be necessary, the index will be increased. If you load a new dataset to the transmission control unit, the dataset identification data is changed automatically.
| Entire control system
| The entire control system identification data includes the version, the appropriate material number and the manufacturing date. The entire control system version name always comprises of the "ECU" for the entire control system, the hardware used (E300.1-), the software version (D5.2.0.0-) and the dataset number (08154701). The identifier "150." and the dataset number yield the material number. The date of the entire control system indicates when the software and the dataset were loaded to the transmission control unit and thus became a entire control system. If you load a new software or a new dataset to the transmission control unit, a new entire control system with a new date will be created automatically.
| Loader
| The loader is a software in the transmission control unit that has the function to load function software and datasets to the transmission control unit. The existence of a loader is therefore inevitable for putting a transmission control unit into operation. The loader designation starts with an "F" (for "flash"), followed by the version number. Two different loaders are currently available. Version F04.04.07-u for transmission control units of the E300 series and version F05.05.03-u for the E300.1 series.
The hardware, software, dataset and entire control system designations are so-called descriptive numbers. Every designation allows to read the conditions that must be met for correct functioning. The function software is always developed for a specific hardware that is indicated by the designation E300 or E300.1 in the name. Datasets are always created for a specific software that, again, requires a specific hardware. This is why the dataset version always contains the name of the software version including the hardware identifier (e.g., E300.1-D5.2.0.0). The entire control system always requires hardware, software and dataset and it can only be created if all three components are compatible. That is why the name of the entire control system always includes the complete hardware-software-dataset identification. If you attempt to put a entire control system with incompatible components into operation, this can already be seen in the identification data. The transmission system will respond to this attempt with the "forced neutral" condition.
| Component:
> Component | Version | Material number | Date | Serial number |
> Entire control system | ECU-E300.1-D5.2.0.0-08154701 | 150.0154701 | 2006-12-01 | 10355 |
> Transmission | D854.5 C3KT2R2-W50 8.5 | D854.5 C3KT2R2-W50 8.5 | 2006-09-29 | 500350 |
> Gear range selector | ECU-E330.01-G01.03-6814613 | ECU-E330.01-G01.03-6814613 | 2006-05-12 | 1750 |
| Entire control system
| The entire control system identification data includes the version, the appropriate material number and the manufacturing date. The entire control system version name always comprises of the "ECU" for the entire control system, the hardware used (E300.1-), the software version (D5.2.0.0-) and the dataset number (08154701). The identifier "150." and the dataset number yield the material number. The date of the entire control system indicates when the software and the dataset were loaded to the transmission control unit and thus became a entire control system. If you load a new software or a new dataset to the transmission control unit, a new entire control system with a new date will be created automatically.
| Transmission
| The transmission identification data includes the transmission version, the material number, the manufacturing date and the transmission serial number. The version number and the material number are always identical. For further information on the transmission version, please see: DIWA.5 modules and rating plate. The transmission identification data is read by the transmission control unit from the TIM (Transmission Identification Module) when the transmission is activated.
| Gear range selector
| The gear range selector identification data includes the gear range selector version, the material number, the manufacturing date and the serial number. The gear range selector version number always includes "ECU" for electronic control unit, the hardware identifier (e.g., E330.01), the gear range selector software version (e.g., G01.03) and a consecutive number. Communication between the gear range selector and the transmission control unit is always done via the CAN bus. In the event of communication problems (entry in the event memory), the identification data of the gear range selector will not be displayed.
| Identification data - raw data table with scaling table:
| While the above specifications display all the Voith identification data in formatted form, the raw data table contains all the identification data including OEM-specific data. The output of the identification raw data table can be switched ON or OFF in the ALADIN Setup. For further information, please see: Report setup. The scaling table is formatted according to KWP2000. This includes an offset, the LId (Local Identifier / what data area), the format (e.g., ASCII or BCD) and the length of the contents (identification data). The LId is helpful for quickly finding a value in the raw value table. It has been standardized in such a way that the VIN (vehicle identification number) always has the LId 90. All LIds that are not used are referred to as "identifiers".
> Scaling table |
> e.g., 04 | e.g., 86 | e.g., 6F | 6F | 62 |
> Offset | LId | Format | Data length |
| LIds not used by Voith:
| The identification data is defined up to LId '9F' according to KWP. All higher LIds are identified additionally by Voith.
> LId | Identifier | Content / example | Note |
> 8A | ECU system supplier name | VOITH | Manufacturer of the transmission control unit (E300 / E300.1) |
> 8B | ECU manufacturing date | 2006-12.01 | Entire control system manufacturing date |
> 8C | ECU serial number | 10355 | Transmission control unit serial number |
> 8D | ECU Identification | ECU-E300.1-D5.2.00-081547110 | Entire control system version number |
> 8E | Device type / diagnostic object | DIWA.5 | Device type / diagnostic object |
> 8F | ECU programming date | 2006-12-01 | Entire control system manufacturing date |
> 8F | Software µC1 manufacturing date | 2006-09-29 | Software manufacturing date |
> 8F | Software µC2 programming date | 2006-09-29 | Transmission manufacturing date (TIM programming). For further information, please see: TIM |
> 8F | Dataset manufacturing date | 2006-08-25 | Dataset manufacturing date |
> 8F | Hardware manufacturing date | 2006-06-19 | Transmission control unit manufacturing date |
> 92 | Hardware identification | 150.00001321 | Transmission control unit material number |
> 93 | Hardware version | E300.1 | Transmission control unit version |
> 94 | Software µC1 identification | 150.00261410 | Software material number |
> 95 | Software µC1 version | E300.1-D5.2.0.0 | Software version |
> | LIds defined additionally by Voith: |  |  |
> B1 | Loader version | F05.05.03-U | Loader in the transmission control unit |
> B2 | Dataset information | Series | Information on the dataset |
> B3 | Hardware information | 36MHz V1 | Information on the transmission control unit |
> B4 | Dataset identification | 150.00263201 | Dataset material number |
> B5 | Dataset version | E300.1-D5.2.0.0-081547110 | Dataset version |
> B6 | Gear range selector identification | ECU-E330.01-G01.03-6814613 | Gear range selector material number |
> B7 | Gear range selector serial number | 1750 | Gear range selector serial number |
> B8 | Gear range selector manufacturing date | 2006-05-12 | Gear range selector manufacturing date |
> B9 | Gear range selector Version | ECU-E330.01-G01.03-6814613 | Gear range selector version |
> BA | Object identification | D854.5 C3KT2R2-W50 8.5 | Transmission material number / version |
> BB | Object serial number | 500350 | Transmission serial number |
> BC | Object manufacturing date | 2006-09-29 | Transmission manufacturing date |
> BD | Object distance [km] |  |  |
> BE | Object information |  | Information on the transmission |
> BF | Dataset parameter OEM_ID_ |  |  |
| LIds used by OEMs:
| The KWP prescribes specific contents in defined LIds for all OEMs.
> LId | Identifier | Content / example | Note |
> 90 | VIN (Vehicle Identification Number) |  | Replaces the former chassis number. For further information, please see: VIN |
> 91 | VehicleManufacturerECUHardwareNumber |  |  |
> 96 | ExhaustRegulationOrTypeApprovalNumber |  |  |
> 97 | SystemNameOrEngineType | DIWA.5_E300.1_VOITH | Transmission or engine |
> 98 | RepairShopCodeOrTesterSerialNumber |  |  |
| Identification data cannot be deleted.
| How to adjust the report contents:
In the ALADIN Setup, you can configure what is displayed and how it is displayed in the ECU report. Click Setup > Report in the main window. For further information, please see: Report setup.
| Further topics:
More information on: Upload More information on: User level More information on: TIM More information on: DIWA.5 modules and rating plate More information on: Gear range selector More information on: Setup More information on: VIN More information on: KWP2000 More information on: Dataset More information on: Voith customer service index More information on: FAQ Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)