# Program properties Prior to using the Recorder for measuring data acquisition, we recommend adjusting the Program Properties to suit your requirements. These settings are especially important for communication with a Voith control unit. Communication via the serial interface (COM1) in connection with a serial K-line interface is the standard configuration.
| How to open the Program Properties:
Click File > Program Properties in the Recorder. The Setup window appears.
| How to save the changes in the Program Properties:
To ensure that all changes of the Recorder setup are transferred, you must exit the Setup window using the OK button. If you want to discard the changes, click the Cancel button.
| Common tab:
The general settings are made in the Common tab. This tab contains all settings for enabling your Recorder version (Registration Information) and the general options (Options). A release is not required for the current Recorder version. The general options Send Measurement to: Here you can enter any e-mail address to send a measuring file directly from the Recorder. Preferred Language: Here you can set your preferred program language. The following languages are available: German, English, Spanish, French, Italian and Russian. Play Music, Play Sounds: Here you can activate the output of acoustic messages.
| Directories tab:
> The "Directories" tab defines the directories to be used by the Analyzer. If you want to change a directory, click the corresponding button, e.g.: Recordings. The "Browse" dialog box then appears. Navigate to the required directory and exit the dialog box with "OK". If you do not want to change a directory, exit the dialog box using the Cancel button. Alternatively, you can enter the directory name in the text field to the right of the corresponding button. Directories used:
> Recordings | Your new measuring files are saved in this directory.
> Templates | This directory contains the measuring template files.
> VarFiles | This directory contains the so-called VarFiles.
> Dataset | This directory contains the datasets for the control unit software versions.
> Temporary Files | This directory stores the Analyzer files that are created and required during the runtime.
> Fault Memory Help | This directory contains the fault help for the event memory of the E300 / E300.1 transmission control units.
> VarFile Help | This directory contains the HTML help for the dataset constants.
| Note! When changing directories, please make sure you have the appropriate read and write rights for these directories. Changes in the directory structure may affect the program execution.
| Recording tab:
> > This tab is used to make the settings for communication with the control units and the measuring equipment. ECU Communication with a control unit is configured in this area. - When using a serial K-line interface (level converter): COM Port: Here you can set the RS232 port (COM port) the K-line interface has been connected to. Baudrate (KWP): Here you can set the Baud rate to be used for communication between the PC and the control unit. "Default" has been preset. This setting enables communication with any transmission control unit irrespective of the vehicle manufacturer. You can select the "Network" entry additionally. This causes the Recorder to record the data via a DIANA5 server. You can also set your PC in such a way that it works as a DIANA5 server. For this purpose, select the "Activate DIANA5 Server". For further information on sending measuring data via a network, please refer to: Using the Network function in the Recorder. Maximum possible Baud rate:
> > E200 | 38400
> > E300 | 115200
> > E300.1 | 57600
> > > - When using the K-line USB interface: If you want to establish communication with a control unit using the Voith K-line USB interface, activate the option "Use VOITH K-Line-USB-Interface".
> > > | Note! The USB interface can be used with transmission control units of the E300 / E300.1 series only. Before you can use the USB interface, you must have installed the appropriate driver first.
> > For further information on the K-line interface, please see: K-line interfaces. GPS Receiver This function can only be used with restrictions in the current version. MIDI Controller This function can only be used with restrictions in the current version. IRMA This function can only be used with restrictions in the current version. Additional options:
> > Auto Record (Datalogger Mode) | This option provides the following functions: The Recorder attempts to start communication with the measuring devices until it is successful. This process can only be cancelled by exiting the Recorder. When a measuring template file is loaded, the Recorder immediately goes to the recording mode. If communication is interrupted for more than 10 seconds during an ECU measurement, a new measuring file will be created. The program does not query before saving measuring files.
> > Activate DIANA5 Server | Activates the Recorder as a DIANA5 measuring server.
> > Calibrate A/D on Startup | Calibrates the A/D converters at program start. This function can only be used with restrictions in the current version.
> > Ask for Recording Details | Measuring information is requested prior to recording measuring data.
> > Use VOITH K-Line-USB-Interface | The USB K-line interface is used instead of a serial K-line interface.
> > Minimize ECU-Data-Download | Extended ECU contents are not downloaded during the download of ECU data from a control unit (e.g., RIO or maintenance data). This considerably enhances the upload.
| Panel tab:
> > The Panel tab can be used to define the graphical display of the Recorder. Background: Defines the background color in the effective range of the Recorder. Bitmap: Here you can select an individual wallpaper for the effective range of the Recorder. Alignment: Here you can select the display of the wallpapers in the Recorder. You can select:
> > Layout | Description
> > Centered1 | The wallpaper is centered. The current frame color is used as a background color.
> > Centered2 | The wallpaper is centered. The color in the top left edge of the wallpaper is used as a background color.
> > Stretched | The wallpaper is stretched to fill the complete effective range.
> > Tiled | The wallpaper is arranged as tiles.
VI Title Size: Font size of the headings of the virtual measuring instruments in the Recorder. VI Title Colors: Graphical display of the virtual measuring instruments in the Recorder: Reset: The standard settings of the tab are restored. Frame Color: The frame color displayed. Title Color: The heading color. Title Back: The background color of the headings. Value Color: The color of the instrument designation. Value Back: The background color of the instrument designation.
| PLC tab:
The PLC settings are used to access the flag area of the PLC controller made by Beckhoff. This function is not available in the current version. How to proceed: Using the Recorders
| Further topics:
More information on: Introduction More information on: Installation / removal More information on: Files used & control units supported More information on: Program overview and initial start-up More information on: K-line interfaces for connecting the ECU and the Recorder More information on: Using the Network function in the Recorder Up > © by Voith Turbo GmbH & Co. KG send remarks to Gottfried.Graf@Voith.com (electronic department) or r.theilacker@voith.com (electronic department)