> # Diagnostic functions available The following diagnostic functions are available in ALADIN:
> Diagnostic function | Task / problems |
> Download | Loads function software, dataset or loader to the transmission control unit |
> Upload & Report | Reads and displays the event memory |
> Monitors | Tests sensors, control elements and inputs/outputs |
> Shift program configuration | Sets and reads the shift program configuration |
> TIM configuration | Reads and writes TIM data |
> Reset functions | Resets data in the transmission control unit |
> Drain converter module | Oil level and oil change support |
> Actuator test | Selectively checks the solenoid valves |
> Clear fault memory | Resets / clears the event memory |
> Service data | Enters service data to the PDI |
> Report | Displays and compares transmission data, operating data etc. |
> Scourcer / Report | Checks the CAN messages in the vehicle |
> EOL | EOL configuration |
For the diagnostic functions available in your current user level, please refer to User level.
| Further topics:
More information on: The ALADIN main window More information on: FAQ More information on: ALADIN terms More information on: User level More information on: TOP 10 Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)