# Display the EOL data in the report
The vehicle-specific variables are set at the end of the line during production using EOL parameters and the corresponding diagnostic services. At present, approx. 200 parameters are vehicle-specific in DIWA.5. This is why they are potentially required for a complete EOL configuration.
| The EOL parameterization is available as of transmission software version E300.1-D5.8.0.0.
| Contents of the EOL data report:
> | How to evaluate the EOL parameterization displayed:
> | The report lists all EOL groups that are known with the corresponding parameters. The following is displayed for each parameter:
> | Min | Lowest adjustable value |
> | Max | Highest adjustable value |
> | Default | Original value from the dataset |
> | Value | Currently used by the control unit |
> | Unit | Unit of the value |
> | Difference | Indicates whether there is a difference to the dataset. |
| How to adjust the report contents:
In the ALADIN Setup, you can configure what is displayed and how it is displayed in the ECU report. Click Setup > Report in the main window. For further information, please see: Report setup.
| How to change adaptation data:
If you want to change the complete EOL data, use the Voith EOL Manager. For further information, please see: EOL Manager.
| Further topics:
More information on: Upload More information on: Setup More information on: ECU files More information on: User level More information on: EOL More information on: FAQ Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)