# Version-specific differences in the diagnostic functions of ALADIN and the function software The function software of the DIWA.5 transmission is constantly being developed. Specific diagnostic functions are therefore available only from a certain transmission software version.
| Overview of supported diagnostic functions in the DIWA.5 software versions
Diagnostic function | As of function software |
Transmission control unit | E300 | E300.1 |
Display of datasets in the report | E300-D2.2.0.0 | E300.1-D5.0.0.0 |
Early-warning system (basic) | E300-D2.2.0.0 | E300.1-D5.0.0.0 |
Early-warning system (full) | E300-D2.5.1.0 | E300.1-D5.2.0.0 |
Flashing of gear range selector | E300-D2.2.0.0 | E300.1-D5.0.0.0 |
Shift program configuration / configuring the SP-SEL position | E300-D2.4.0.0 | E300.1-D5.0.0.0 |
Shift program configuration / display of the SP-SEL switch |  | E300.1-D5.0.0.0 |
TIM support / Write to TIM |  | E300.1-D5.0.0.0 |
RESET functions |  | E300.1-D5.0.0.0 |
Drain converter |  | E300.1-D5.2.0.0 |
History storage |  | E300.1-D5.2.0.0 |
Scourcer |  | E300.1-D5.2.0.0 |
Resetting the slip monitoring function |  | E300.1-D5.5.0.0 |
EOL |  | E300.1-D5.8.0.0 |
Shift program configuration / SensoTop |  | E300.1-D5.8.0.0 |
| Further topics
More information on: User level More information on: History storage More information on: Actuator test More information on: Drain converter More information on: Shift program configuration More information on: Display of SP_SEL switch More information on: Oil ageing index More information on: FAQ Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)